

RMBOOTSECT v1.2.0  (c)2008 RM Education plc [SSi]
====================================================

Converts between an NTLDR (XP) and BootMgr (Vista\WinPE v2) boot loader

Usage:
 RMBootSect  [/nt52 | /MSDOS]  <drive_letter>:   [/debug] [/nowrite] [/ZIP]

Examples:
 RMBootSect D:        (to write a Vista compatible boot sector)
 RMBootSect /nt52 D:  (to write an XP compatible boot sector)
 RMBootSect /MSDOS D: /ZIP (to write an MSDOS FAT16 compatible boot sector)

Notes:
 For WinPE bootable USB flash devices, partition using WinPE\Vista first.
 RMBootSect modifies FAT/FAT32 volumes to work as WinPE bootable drives.
 /MSDOS option only valid for FAT16 (FAT) partitions.
 Errorlevel 0 returned on success.
